**Pixelle Specialty Solutions – Stevens Point Mill**

**Contractor Test - 2022**

**PRINT the following:**

Print Name Legibly\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Company\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Email Contact\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Cell Phone\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Pixelle Contact Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**For each question, please select the best single answer from the choices below:**

1. I have to take personal responsibility to keep myself and my co-workers safe?
	1. True
	2. False
2. Am I allowed to wear my wedding ring under my glove?
	1. Yes
	2. No. No rings, necklaces or dangling earrings are allowed on the operating floor.
3. Beards longer than 4 inches below the chin must be restrained with a beard restraint.
	1. True
	2. False
4. Wristwatches with bands that continue under the face are not allowed in production areas. Watchbands with breakaway pins are acceptable.
	1. True
	2. False
5. It is good practice to identify my nearest exit prior to starting my assigned job.
	1. True
	2. False
6. If I am not familiar with the equipment I am going to work on and I am not sure where I should lockout, I should:
	1. Give it my best guess and just attach my lock
	2. Rely on the opinion of a co-worker
	3. Stop, request a mill operator or mill supervisor to show me what the energy sources are and where to place my lock
7. As a contractor, if I have information on a flash drive, external hard drive or other portable storage device I can simply attached it to a Pixelle computer
	1. True
	2. False – I need to contact Pixelle IT and have a full scan done on the device
8. A hot work permit is required for:
	1. Welding
	2. Using a torch
	3. Soldering
	4. Grinding
	5. All of the above
9. \_\_\_\_\_\_\_\_ is a very highly damaging contaminant in pulp and papermaking and it can enter our system anywhere throughout the paper making process. We ask that you monitor and pick up this contaminate if you see it in your work areas.
	1. Plastic
	2. Metal
	3. Cloth
10. Plastic barricade tape shall not be used in the mill, only cloth is permitted. Where can you obtain cloth type barricade tape?
	1. Storeroom
	2. Security Office
11. Prior to bringing chemicals on site, the Contractor will:
	1. Provide SDS for each chemical
	2. Provide an estimate of the quantity of all materials brought on–site
	3. Complete a material inventory form available through the Environmental Department
	4. All of the above
12. Do not dispose of batteries or light bulbs in the mill trash. Bring all used batteries to the \_\_\_\_\_\_\_\_\_\_and ask for assistance in recycling of batteries.
	1. Security Office
	2. Storeroom
	3. Test Lab
13. Used oils must be managed properly according to EPA regulations. Collect all used oil in a closed container. The EPA requires all used oil to be labeled as:
	1. Used Oil
	2. Waste Oil
14. Hard hats will be worn:
	1. Only in the boilerhouse
	2. On all maintenance down days and outages.
15. Safety shields are required on all safety glasses.
	1. True
	2. False
16. Hearing protection is mandatory:
	1. Only on down days and when the area is noisy
	2. In all operating areas including machine down days
17. If you hear the evacuation alarm you should evacuate the building and meet:
	1. Along the edge of the river
	2. In the corner of the parking lot by the yellow pole building
	3. In the visitor parking lot
18. The maximum speed limit in all parking lots is \_\_\_\_\_\_mph.
	1. 35
	2. 15
	3. 25
19. If there is an emergency and you need immediate help what is the very first thing you should do?
	1. Use your cell phone to call for help
	2. Pull the nearest fire alarm box as this notifies the Mill’s emergency response team that you need help.
	3. Scream very loud
20. Hi-visibility vests/shirts are required in Stock Preparation and the warehouse due to tow motor traffic.
	1. True
	2. False
21. Fall protection is required at an unprotected height of \_\_\_\_\_\_\_\_\_\_\_\_feet.
	1. 2
	2. 4
	3. 6
22. Contractors entering a confined space shall supply their own:
	1. Air quality testing/monitoring equipment
	2. A confined space entry permit
	3. Ventilation and lighting equipment
	4. A harness and lifeline
	5. All of the above
23. If I am in a hurry I can cut across and walk between two connected rail cars.
	1. True
	2. False
24. If a hazardous waste spill occurs:
	1. Wash it down the nearest process sewer
	2. Stop the release if this can be done safely and contact the mill environmental people
	3. Contact your project manager who will inform the appropriate Pixelle team member
25. Lockout/Tagout is necessary whenever you are performing service or maintenance around any machine where you could be injured by:
	1. Unexpected start-up of the equipment
	2. Release of stored energy
	3. All of the above.
26. Only this type of ladder is allowed on Pixelle sites:
	1. Metal
	2. Fiberglass reinforced plastic
	3. Plastic
27. What type of barricade can you enter if you are aware of the identified hazard?
	1. Yellow Caution Tape
	2. Red Danger Tape
28. Under what circumstances may a contractor employee dispose of waste at the Stevens Point mill
	1. In order to dispose of wastes, the contract employee only has to find the proper location
	2. In order to dispose of wastes, the contract employee must have prior approval except for general trash (ex. Lunch bags, beverage containers, etc.)
29. Portable electrical equipment and extension cords must be inspected prior to usage and must be grounded with a three-prong type plug.
	1. True
	2. False
30. All combustibles must be removed at a distance of at least\_\_\_\_\_\_\_\_\_\_feet from a hot work area or curtains/shields installed that go all the way to the floor.
	1. 25
	2. 35
	3. 6
	4. 60
31. If you want to cross a blue line on the floor you need to:
	1. Be accompanied by an authorized team member;
	2. Receiving instruction about the hazards of the moving equipment in the area from the authorized team member; or
	3. After the equipment is locked out per LOTO procedures.
	4. All of the above

Revision Summary: 12/21/17 New test questions.

2-6-18 Added: Print Name Legibly. 11/21/19 – new question. 10/6/2020 – Fixed an answer key error.

Document Owner: Safety Advocate